# Forewords

This document applies to the NurseCall L051TX\_RAC80 FW programming, dedicated to the RAC80 and UPCBA80 products.

Files are supplied in binary format.

# L051TX\_RAC80 firmware:

Software SAP#: T.040.001.547

Software SAP Description: Software RAC80

Software information to be printed  None

## Binary firmware version details:

File format: binary

Version: NC\_08.A00.02.1483

Build date: 15.11.2022

Compiler version IAR EWARM 8.50.6

File Name: NC\_08.A00.02.1483.bin

MD5 Checksum: B2A61549ED366C30D85B05C27E60BA6C

Remark: None

## Change History:

|  |  |  |
| --- | --- | --- |
| SW Version | Build date | Description |
| 08.A00.01.1396 | 04.06.2021 | Ready for Ramp-up production |
| 08.A00.01.1422 | 01.11.2021 | Fixed character problem in Production initialization |
| 08.A00.02.1483 | 15.11.2022 | LOW BAT THRESHOLD forced to Factory value ADC closing reviewed after Battery measurement (consumption) |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |